= LSM9DS1 Library for Arduino =

image:https://github.com/arduino-libraries/Arduino_LSM9DS1/workflows/Compile%20Examples/badge.svg["Compile Examples Status", link="https://github.com/arduino-libraries/Arduino_LSM9DS1/actions?workflow=Compile+Examples"] image:https://github.com/arduino-libraries/Arduino_LSM9DS1/workflows/Spell%20Check/badge.svg["Spell Check Status", link="https://github.com/arduino-libraries/Arduino_LSM9DS1/actions?workflow=Spell+Check"]

Allows you to read the accelerometer, magnetometer and gyroscope values from the LSM9DS1 IMU on your Arduino Nano 33 BLE Sense.

== License ==

Copyright (c) 2019 Arduino SA. All rights reserved.

This library is free software; you can redistribute it and/or
modify it under the terms of the GNU Lesser General Public
License as published by the Free Software Foundation; either
version 2.1 of the License, or (at your option) any later version.

This library is distributed in the hope that it will be useful,
but WITHOUT ANY WARRANTY; without even the implied warranty of
MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the GNU
Lesser General Public License for more details.

You should have received a copy of the GNU Lesser General Public
License along with this library; if not, write to the Free Software
Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA 02110-1301 USA
