| ThreeSpace API 2 2.0.6.1 Serial wrapper for YEI 3-Space Sensor Protocol

- Main Page
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Data Fields
TSS_ComInfo Struct Reference

`#include <yei_threespace_api.h>`

## Data Fields
TSS_Type | device_type
unsigned int | serial_number
char | firmware_version [13]
char | hardware_version [33]
TSS_Firmware_Compatibility | fw_compatibility

## Detailed Description

A structure that contains information about the connected 3-Space device.

Definition at line 284 of file yei_threespace_api.h.

## Field Documentation

TSS_Type device_type

The type of 3-Space device connected through the com port.

Definition at line 286 of file yei_threespace_api.h.

unsigned int serial_number

The serial number for the 3-Space device connected through the com port.

Definition at line 287 of file yei_threespace_api.h.

char firmware_version[13]

The version of the firmware installed on the connected 3-Space device.

Definition at line 288 of file yei_threespace_api.h.

char hardware_version[33]

The hardware revision and type of the connected 3-Space device.

Definition at line 289 of file yei_threespace_api.h.

TSS_Firmware_Compatibility fw_compatibility

Firmware compatibility level (Note level may be lower than current if no functional changes were made).

Definition at line 290 of file yei_threespace_api.h.

The documentation for this struct was generated from the following file:

- yei_threespace_api.h